# Static Call Graph for image .\Obj\ethernet_bootloader.axf

#<CALLGRAPH># ARM Linker, 5060422: Last Updated: Mon Mar 04 12:33:49 2019

### Maximum Stack Usage = 216 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

SystemInit ⇒ Board_SystemInit ⇒ Board_SetupClocking ⇒ Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- UnHandled_Vector ⇒ UnHandled_Vector
- ADC0_IRQHandler ⇒ ADC0_IRQHandler
- Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz
- Chip_Clock_GetDivRate ⇒ Chip_Clock_GetClockInputHz

  ### Function Pointers

  - ADC0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - ADC1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - ADCHS_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - ATIMER_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - BusFault_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - CAN0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - CAN1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - DAC_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - DMA_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - DebugMon_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - ETH_IRQHandler from comms.o(i.ETH_IRQHandler) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - EVRT_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - FLASH_EEPROM_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GINT0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GINT1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO2_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO3_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO4_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO5_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO6_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - GPIO7_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - HardFault_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - I2C0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - I2C1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - I2S0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - I2S1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - LCD_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - M0APP_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - M0SUB_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - MCPWM_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - MemManage_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - NMI_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - PendSV_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - QEI_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - RIT_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - RTC_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - Reset_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SCT_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SDIO_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SGPIO_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SPIFI_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SPI_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SSP0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SSP1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SVC_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SysTick_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - SystemInit from sysinit.o(i.SystemInit) referenced from keil_startup_lpc18xx43xx.o(.text)
  - TIMER0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - TIMER1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - TIMER2_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - TIMER3_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UART0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UART1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UART2_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UART3_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - USB0_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - USB1_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - UnHandled_Vector from keil_startup_lpc18xx43xx.o(.text) referenced 7 times from keil_startup_lpc18xx43xx.o(RESET)
  - UsageFault_Handler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - WDT_IRQHandler from keil_startup_lpc18xx43xx.o(.text) referenced from keil_startup_lpc18xx43xx.o(RESET)
  - __main from __main.o(!!!main) referenced from keil_startup_lpc18xx43xx.o(.text)
  - localMsDelay from comms.o(i.localMsDelay) referenced from comms.o(i.init_comms)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ enter_isp ⇒ isp_cmd_loop ⇒ exec_isp_cmd ⇒ write_to_ram ⇒ getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  UnHandled_Vector (Thumb, 2 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> UnHandled_Vector
  [Called By]
  - >> UnHandled_Vector
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Calls]

  - >> ADC0_IRQHandler
  [Called By]
  - >> ADC0_IRQHandler
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  ADCHS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  ATIMER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  CAN0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  CAN1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  EVRT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  FLASH_EEPROM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  GPIO7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  I2S0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  I2S1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  LCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  M0APP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  M0SUB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SCT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SGPIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SPIFI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  USB0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  USB1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_startup_lpc18xx43xx.o(.text))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, keil_startup_lpc18xx43xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __aeabi_memcpy (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text))
  [Called By]

  - >> getline_ex
  - >> comm_handshake

  __rt_memcpy (Thumb, 138 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4

  _memcpy_lastbytes (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_v6.o(.text), UNUSED)

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_memclr4
  [Called By]
  - >> InitDescriptors

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 78 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  Board_SystemInit (Thumb, 16 bytes, Stack size 8 bytes, board_sysinit.o(i.Board_SystemInit))
  [Stack]

  - Max Depth = 208
  - Call Chain = Board_SystemInit ⇒ Board_SetupClocking ⇒ Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Board_SetupMuxing
  - >> Board_SetupExtMemory
  - >> Board_SetupClocking
  [Called By]
  - >> SystemInit

  Chip_GPIO_Init (Thumb, 2 bytes, Stack size 0 bytes, gpio_18xx_43xx.o(i.Chip_GPIO_Init))
  [Called By]

  - >> Board_Init

  ETH_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, comms.o(i.ETH_IRQHandler))
  [Address Reference Count : 1]

  - keil_startup_lpc18xx43xx.o(RESET)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)
  [Called By]

  - >> __rt_memcpy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  __rt_memcpy_w (Thumb, 100 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  _memcpy_lastbytes_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_w.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  Board_Init (Thumb, 62 bytes, Stack size 8 bytes, board.o(i.Board_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = Board_Init ⇒ Board_LED_Init
  [Calls]
  - >> Chip_SCU_PinMuxSet
  - >> Board_LED_Init
  - >> Chip_GPIO_Init
  [Called By]
  - >> enter_isp

  Board_SetupClocking (Thumb, 158 bytes, Stack size 16 bytes, board_sysinit.o(i.Board_SetupClocking))
  [Stack]

  - Max Depth = 200
  - Call Chain = Board_SetupClocking ⇒ Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_SetupCoreClock
  - >> Chip_Clock_SetDivider
  - >> Chip_Clock_SetBaseClock
  [Called By]
  - >> Board_SystemInit

  Board_SetupExtMemory (Thumb, 82 bytes, Stack size 8 bytes, board_sysinit.o(i.Board_SetupExtMemory))
  [Stack]

  - Max Depth = 144
  - Call Chain = Board_SetupExtMemory ⇒ Chip_EMC_Static_Init ⇒ Chip_Clock_GetEMCRate ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_EMC_Static_Init
  - >> Chip_EMC_Init
  - >> Chip_EMC_Dynamic_Init
  - >> Chip_Clock_Enable
  - >> Chip_Clock_EnableOpts
  [Called By]
  - >> Board_SystemInit

  Board_SetupMuxing (Thumb, 58 bytes, Stack size 8 bytes, board_sysinit.o(i.Board_SetupMuxing))
  [Stack]

  - Max Depth = 24
  - Call Chain = Board_SetupMuxing ⇒ Chip_SCU_SetPinMuxing
  [Calls]
  - >> Chip_SCU_SetPinMuxing
  [Called By]
  - >> Board_SystemInit

  Chip_Clock_DisableMainPLL (Thumb, 14 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_DisableMainPLL))
  [Called By]

  - >> Chip_Clock_SetupMainPLLMult

  Chip_Clock_Enable (Thumb, 46 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_Enable))
  [Called By]

  - >> Board_SetupExtMemory
  - >> Chip_TIMER_Init

  Chip_Clock_EnableCrystal (Thumb, 62 bytes, Stack size 8 bytes, clock_18xx_43xx.o(i.Chip_Clock_EnableCrystal))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_Clock_EnableCrystal
  [Called By]
  - >> Chip_SetupCoreClock

  Chip_Clock_EnableOpts (Thumb, 52 bytes, Stack size 16 bytes, clock_18xx_43xx.o(i.Chip_Clock_EnableOpts))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_Clock_EnableOpts
  [Called By]
  - >> Chip_ENET_Init
  - >> Board_SetupExtMemory

  Chip_Clock_GetBaseClock (Thumb, 32 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetBaseClock))
  [Called By]

  - >> Chip_Clock_GetBaseClocktHz

  Chip_Clock_GetBaseClocktHz (Thumb, 18 bytes, Stack size 16 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetBaseClocktHz))
  [Stack]

  - Max Depth = 80
  - Call Chain = Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetClockInputHz
  - >> Chip_Clock_GetBaseClock
  [Called By]
  - >> Chip_Clock_GetRate

  Chip_Clock_GetClockInputHz (Thumb, 182 bytes, Stack size 16 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetClockInputHz))
  [Stack]

  - Max Depth = 64
  - Call Chain = Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetMainPLLHz
  - >> Chip_Clock_GetDivRate
  [Called By]
  - >> Chip_Clock_SetupMainPLLMult
  - >> Chip_Clock_SetupMainPLLHz
  - >> Chip_Clock_GetMainPLLHz
  - >> Chip_Clock_GetBaseClocktHz
  - >> Chip_Clock_GetDivRate

  Chip_Clock_GetDividerDivisor (Thumb, 18 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetDividerDivisor))
  [Called By]

  - >> Chip_Clock_GetDivRate

  Chip_Clock_GetDividerSource (Thumb, 26 bytes, Stack size 0 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetDividerSource))
  [Called By]

  - >> Chip_Clock_GetDivRate

  Chip_Clock_GetEMCRate (Thumb, 38 bytes, Stack size 16 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetEMCRate))
  [Stack]

  - Max Depth = 120
  - Call Chain = Chip_Clock_GetEMCRate ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetRate
  [Called By]
  - >> Chip_EMC_Static_Init
  - >> Chip_EMC_Dynamic_Init

  Chip_Clock_GetMainPLLHz (Thumb, 110 bytes, Stack size 48 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetMainPLLHz))
  [Stack]

  - Max Depth = 48 + In Cycle
  - Call Chain = Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetClockInputHz
  [Called By]
  - >> Chip_Clock_GetClockInputHz

  Chip_Clock_GetRate (Thumb, 78 bytes, Stack size 24 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetRate))
  [Stack]

  - Max Depth = 104
  - Call Chain = Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetBaseClocktHz
  - >> Chip_Clock_FindBaseClock
  [Called By]
  - >> StopWatch_Init
  - >> SystemCoreClockUpdate
  - >> Chip_Clock_GetEMCRate

  Chip_Clock_SetBaseClock (Thumb, 64 bytes, Stack size 16 bytes, clock_18xx_43xx.o(i.Chip_Clock_SetBaseClock))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_Clock_SetBaseClock
  [Called By]
  - >> Board_SetupClocking
  - >> Chip_SetupCoreClock

  Chip_Clock_SetDivider (Thumb, 64 bytes, Stack size 12 bytes, clock_18xx_43xx.o(i.Chip_Clock_SetDivider))
  [Stack]

  - Max Depth = 12
  - Call Chain = Chip_Clock_SetDivider
  [Called By]
  - >> Board_SetupClocking

  Chip_Clock_SetupMainPLLHz (Thumb, 190 bytes, Stack size 56 bytes, clock_18xx_43xx.o(i.Chip_Clock_SetupMainPLLHz))
  [Stack]

  - Max Depth = 160
  - Call Chain = Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_SetupMainPLLMult
  - >> Chip_Clock_GetClockInputHz
  - >> Chip_Clock_TestMainPLLMultiplier
  [Called By]
  - >> Chip_SetupCoreClock

  Chip_Clock_SetupMainPLLMult (Thumb, 160 bytes, Stack size 40 bytes, clock_18xx_43xx.o(i.Chip_Clock_SetupMainPLLMult))
  [Stack]

  - Max Depth = 104
  - Call Chain = Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetClockInputHz
  - >> Chip_Clock_DisableMainPLL
  [Called By]
  - >> Chip_Clock_SetupMainPLLHz

  Chip_EMC_Dynamic_Init (Thumb, 22 bytes, Stack size 16 bytes, emc_18xx_43xx.o(i.Chip_EMC_Dynamic_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = Chip_EMC_Dynamic_Init ⇒ Chip_Clock_GetEMCRate ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> initDynMem
  - >> Chip_Clock_GetEMCRate
  [Called By]
  - >> Board_SetupExtMemory

  Chip_EMC_Init (Thumb, 40 bytes, Stack size 8 bytes, emc_18xx_43xx.o(i.Chip_EMC_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_EMC_Init
  [Called By]
  - >> Board_SetupExtMemory

  Chip_EMC_Static_Init (Thumb, 22 bytes, Stack size 16 bytes, emc_18xx_43xx.o(i.Chip_EMC_Static_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = Chip_EMC_Static_Init ⇒ Chip_Clock_GetEMCRate ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> initStaticMem
  - >> Chip_Clock_GetEMCRate
  [Called By]
  - >> Board_SetupExtMemory

  Chip_ENET_Init (Thumb, 122 bytes, Stack size 8 bytes, enet_18xx_43xx.o(i.Chip_ENET_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = Chip_ENET_Init ⇒ Chip_Clock_EnableOpts
  [Calls]
  - >> Chip_RGU_TriggerReset
  - >> Chip_RGU_InReset
  - >> Chip_Clock_EnableOpts
  - >> Chip_ENET_SetupMII
  [Called By]
  - >> init_comms

  Chip_ENET_SetDuplex (Thumb, 22 bytes, Stack size 0 bytes, enet_18xx_43xx.o(i.Chip_ENET_SetDuplex))
  [Called By]

  - >> init_comms

  Chip_ENET_SetSpeed (Thumb, 22 bytes, Stack size 0 bytes, enet_18xx_43xx.o(i.Chip_ENET_SetSpeed))
  [Called By]

  - >> init_comms

  Chip_ENET_SetupMII (Thumb, 14 bytes, Stack size 8 bytes, enet_18xx_43xx.o(i.Chip_ENET_SetupMII))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_ENET_SetupMII
  [Called By]
  - >> Chip_ENET_Init

  Chip_ENET_StartMIIRead (Thumb, 20 bytes, Stack size 0 bytes, enet_18xx_43xx.o(i.Chip_ENET_StartMIIRead))
  [Called By]

  - >> lpcPHYStsPoll
  - >> lpc_mii_read

  Chip_ENET_StartMIIWrite (Thumb, 26 bytes, Stack size 0 bytes, enet_18xx_43xx.o(i.Chip_ENET_StartMIIWrite))
  [Called By]

  - >> lpc_mii_write

  Chip_GPIO_SetPinDIR (Thumb, 62 bytes, Stack size 12 bytes, gpio_18xx_43xx.o(i.Chip_GPIO_SetPinDIR))
  [Stack]

  - Max Depth = 12
  - Call Chain = Chip_GPIO_SetPinDIR
  [Called By]
  - >> lpc_phy_init

  Chip_RGU_InReset (Thumb, 52 bytes, Stack size 8 bytes, rgu_18xx_43xx.o(i.Chip_RGU_InReset))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_RGU_InReset
  [Called By]
  - >> Chip_ENET_Init

  Chip_RGU_TriggerReset (Thumb, 38 bytes, Stack size 8 bytes, rgu_18xx_43xx.o(i.Chip_RGU_TriggerReset))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_RGU_TriggerReset
  [Called By]
  - >> Chip_ENET_Init

  Chip_SetupCoreClock (Thumb, 138 bytes, Stack size 24 bytes, sysinit_18xx_43xx.o(i.Chip_SetupCoreClock))
  [Stack]

  - Max Depth = 184
  - Call Chain = Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_SetupMainPLLHz
  - >> Chip_Clock_SetBaseClock
  - >> Chip_Clock_EnableCrystal
  [Called By]
  - >> Board_SetupClocking

  Chip_TIMER_Init (Thumb, 18 bytes, Stack size 16 bytes, timer_18xx_43xx.o(i.Chip_TIMER_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_TIMER_Init
  [Calls]
  - >> Chip_TIMER_GetClockIndex
  - >> Chip_Clock_Enable
  [Called By]
  - >> StopWatch_Init

  StopWatch_Init (Thumb, 76 bytes, Stack size 8 bytes, stopwatch_18xx_43xx.o(i.StopWatch_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = StopWatch_Init ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_TIMER_Init
  - >> Chip_Clock_GetRate
  [Called By]
  - >> Timer_init

  StopWatch_Start (Thumb, 8 bytes, Stack size 0 bytes, stopwatch_18xx_43xx.o(i.StopWatch_Start))
  [Called By]

  - >> Timer_init
  - >> Timer_HasTimestampExpired
  - >> Timer_GetTimestamp

  StopWatch_TicksToMs (Thumb, 12 bytes, Stack size 0 bytes, stopwatch_18xx_43xx.o(i.StopWatch_TicksToMs))
  [Called By]

  - >> Timer_HasTimestampExpired
  - >> Timer_GetTimestamp

  SystemCoreClockUpdate (Thumb, 14 bytes, Stack size 8 bytes, chip_18xx_43xx.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 112
  - Call Chain = SystemCoreClockUpdate ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetRate
  [Called By]
  - >> enter_isp

  SystemInit (Thumb, 14 bytes, Stack size 8 bytes, sysinit.o(i.SystemInit))
  [Stack]

  - Max Depth = 216
  - Call Chain = SystemInit ⇒ Board_SystemInit ⇒ Board_SetupClocking ⇒ Chip_SetupCoreClock ⇒ Chip_Clock_SetupMainPLLHz ⇒ Chip_Clock_SetupMainPLLMult ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Board_SystemInit
  [Address Reference Count : 1]
  - keil_startup_lpc18xx43xx.o(.text)

  Timer_DeInit (Thumb, 14 bytes, Stack size 0 bytes, timer.o(i.Timer_DeInit))
  [Called By]

  - >> go_cmd

  Timer_GetTimestamp (Thumb, 14 bytes, Stack size 8 bytes, timer.o(i.Timer_GetTimestamp))
  [Stack]

  - Max Depth = 8
  - Call Chain = Timer_GetTimestamp
  [Calls]
  - >> StopWatch_TicksToMs
  - >> StopWatch_Start
  [Called By]
  - >> getline_ex

  Timer_HasTimestampExpired (Thumb, 52 bytes, Stack size 16 bytes, timer.o(i.Timer_HasTimestampExpired))
  [Stack]

  - Max Depth = 16
  - Call Chain = Timer_HasTimestampExpired
  [Calls]
  - >> StopWatch_TicksToMs
  - >> StopWatch_Start
  [Called By]
  - >> getline_ex

  Timer_init (Thumb, 12 bytes, Stack size 8 bytes, timer.o(i.Timer_init))
  [Stack]

  - Max Depth = 120
  - Call Chain = Timer_init ⇒ StopWatch_Init ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> StopWatch_Start
  - >> StopWatch_Init
  [Called By]
  - >> init_comms

  _sys_exit (Thumb, 6 bytes, Stack size 0 bytes, board.o(i._sys_exit))
  [Called By]

  - >> __rt_exit_exit

  a_to_i (Thumb, 54 bytes, Stack size 12 bytes, isp_iap.o(i.a_to_i))
  [Stack]

  - Max Depth = 12
  - Call Chain = a_to_i
  [Called By]
  - >> write_to_ram
  - >> param_check

  blank_check (Thumb, 206 bytes, Stack size 8 bytes, isp_iap.o(i.blank_check))
  [Stack]

  - Max Depth = 56
  - Call Chain = blank_check ⇒ param_check ⇒ a_to_i
  [Calls]
  - >> param_check
  - >> i_to_a
  - >> iap_entry
  - >> sendline_crlf
  [Called By]
  - >> exec_isp_cmd

  check_isp_entry_pin (Thumb, 46 bytes, Stack size 12 bytes, isp_iap.o(i.check_isp_entry_pin))
  [Stack]

  - Max Depth = 12
  - Call Chain = check_isp_entry_pin
  [Called By]
  - >> main

  chksum16 (Thumb, 52 bytes, Stack size 16 bytes, comms.o(i.chksum16))
  [Stack]

  - Max Depth = 16
  - Call Chain = chksum16
  [Called By]
  - >> sendline_crlf

  comm_handshake (Thumb, 108 bytes, Stack size 56 bytes, comms.o(i.comm_handshake))
  [Stack]

  - Max Depth = 152
  - Call Chain = comm_handshake ⇒ getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> str_cmp
  - >> sendline_crlf
  - >> getline_ex
  - >> getline
  - >> __aeabi_memcpy
  [Called By]
  - >> enter_isp

  comms_process (Thumb, 8 bytes, Stack size 8 bytes, comms.o(i.comms_process))
  [Stack]

  - Max Depth = 16
  - Call Chain = comms_process ⇒ ENET_TXBuffClaim
  [Calls]
  - >> ENET_TXBuffClaim
  [Called By]
  - >> sendline_crlf
  - >> isp_cmd_loop

  compare_mem (Thumb, 146 bytes, Stack size 8 bytes, isp_iap.o(i.compare_mem))
  [Stack]

  - Max Depth = 56
  - Call Chain = compare_mem ⇒ param_check ⇒ a_to_i
  [Calls]
  - >> param_check
  - >> i_to_a
  - >> iap_entry
  - >> sendline_crlf
  [Called By]
  - >> exec_isp_cmd

  copy (Thumb, 192 bytes, Stack size 8 bytes, isp_iap.o(i.copy))
  [Stack]

  - Max Depth = 56
  - Call Chain = copy ⇒ param_check ⇒ a_to_i
  [Calls]
  - >> param_check
  - >> i_to_a
  - >> iap_entry
  - >> sendline_crlf
  [Called By]
  - >> exec_isp_cmd

  decode (Thumb, 18 bytes, Stack size 0 bytes, isp_iap.o(i.decode))
  [Called By]

  - >> uudecode

  decode_length (Thumb, 78 bytes, Stack size 12 bytes, isp_iap.o(i.decode_length))
  [Stack]

  - Max Depth = 12
  - Call Chain = decode_length
  [Called By]
  - >> uudecode

  encode (Thumb, 16 bytes, Stack size 0 bytes, isp_iap.o(i.encode))
  [Called By]

  - >> uuencode

  enter_isp (Thumb, 24 bytes, Stack size 0 bytes, sbl_main.o(i.enter_isp))
  [Stack]

  - Max Depth = 192
  - Call Chain = enter_isp ⇒ isp_cmd_loop ⇒ exec_isp_cmd ⇒ write_to_ram ⇒ getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> isp_cmd_loop
  - >> init_comms
  - >> comm_handshake
  - >> SystemCoreClockUpdate
  - >> Board_Init
  [Called By]
  - >> main

  erase (Thumb, 294 bytes, Stack size 8 bytes, isp_iap.o(i.erase))
  [Stack]

  - Max Depth = 56
  - Call Chain = erase ⇒ param_check ⇒ a_to_i
  [Calls]
  - >> param_check
  - >> i_to_a
  - >> iap_entry
  - >> sendline_crlf
  [Called By]
  - >> exec_isp_cmd

  exec_isp_cmd (Thumb, 378 bytes, Stack size 16 bytes, isp_iap.o(i.exec_isp_cmd))
  [Stack]

  - Max Depth = 160
  - Call Chain = exec_isp_cmd ⇒ write_to_ram ⇒ getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> write_to_ram
  - >> unlock
  - >> read
  - >> prepare_sector
  - >> i_to_a
  - >> go_cmd
  - >> erase
  - >> copy
  - >> compare_mem
  - >> blank_check
  - >> iap_entry
  - >> sendline_crlf
  [Called By]
  - >> isp_cmd_loop

  execute_user_code (Thumb, 8 bytes, Stack size 8 bytes, isp_iap.o(i.execute_user_code))
  [Stack]

  - Max Depth = 8
  - Call Chain = execute_user_code
  [Called By]
  - >> main

  filter (Thumb, 176 bytes, Stack size 12 bytes, comms.o(i.filter))
  [Stack]

  - Max Depth = 12
  - Call Chain = filter
  [Called By]
  - >> getline_ex

  getline (Thumb, 34 bytes, Stack size 32 bytes, comms.o(i.getline))
  [Stack]

  - Max Depth = 96
  - Call Chain = getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> getline_ex
  [Called By]
  - >> write_to_ram
  - >> read
  - >> isp_cmd_loop
  - >> comm_handshake

  getline_ex (Thumb, 258 bytes, Stack size 48 bytes, comms.o(i.getline_ex))
  [Stack]

  - Max Depth = 64
  - Call Chain = getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> Timer_HasTimestampExpired
  - >> Timer_GetTimestamp
  - >> filter
  - >> ENET_RXQueue
  - >> ENET_RXGet
  - >> __aeabi_memcpy
  [Called By]
  - >> getline
  - >> comm_handshake

  go_cmd (Thumb, 86 bytes, Stack size 16 bytes, isp_iap.o(i.go_cmd))
  [Stack]

  - Max Depth = 64
  - Call Chain = go_cmd ⇒ param_check ⇒ a_to_i
  [Calls]
  - >> Timer_DeInit
  - >> param_check
  - >> i_to_a
  - >> sendline_crlf
  [Called By]
  - >> exec_isp_cmd

  i_to_a (Thumb, 74 bytes, Stack size 12 bytes, isp_iap.o(i.i_to_a))
  [Stack]

  - Max Depth = 12
  - Call Chain = i_to_a
  [Called By]
  - >> write_to_ram
  - >> unlock
  - >> read
  - >> prepare_sector
  - >> go_cmd
  - >> exec_isp_cmd
  - >> erase
  - >> copy
  - >> compare_mem
  - >> blank_check
  - >> isp_cmd_loop

  initDynMem (Thumb, 488 bytes, Stack size 40 bytes, emc_18xx_43xx.o(i.initDynMem))
  [Stack]

  - Max Depth = 52
  - Call Chain = initDynMem ⇒ convertTimmingParam
  [Calls]
  - >> getColsLen
  - >> convertTimmingParam
  [Called By]
  - >> Chip_EMC_Dynamic_Init

  initStaticMem (Thumb, 104 bytes, Stack size 24 bytes, emc_18xx_43xx.o(i.initStaticMem))
  [Stack]

  - Max Depth = 36
  - Call Chain = initStaticMem ⇒ convertTimmingParam
  [Calls]
  - >> convertTimmingParam
  [Called By]
  - >> Chip_EMC_Static_Init

  init_comms (Thumb, 252 bytes, Stack size 16 bytes, comms.o(i.init_comms))
  [Stack]

  - Max Depth = 136
  - Call Chain = init_comms ⇒ Timer_init ⇒ StopWatch_Init ⇒ Chip_Clock_GetRate ⇒ Chip_Clock_GetBaseClocktHz ⇒ Chip_Clock_GetClockInputHz ⇒ Chip_Clock_GetMainPLLHz ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> lpc_phy_init
  - >> lpcPHYStsPoll
  - >> Timer_init
  - >> Chip_ENET_SetSpeed
  - >> Chip_ENET_SetDuplex
  - >> Chip_ENET_Init
  - >> InitDescriptors
  - >> ENET_RXQueue
  [Called By]
  - >> enter_isp

  is_div (Thumb, 16 bytes, Stack size 0 bytes, isp_iap.o(i.is_div))
  [Called By]

  - >> param_check

  isp_cmd_loop (Thumb, 286 bytes, Stack size 32 bytes, isp_iap.o(i.isp_cmd_loop))
  [Stack]

  - Max Depth = 192
  - Call Chain = isp_cmd_loop ⇒ exec_isp_cmd ⇒ write_to_ram ⇒ getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> tokenize
  - >> i_to_a
  - >> exec_isp_cmd
  - >> sendline_crlf
  - >> getline
  - >> comms_process
  [Called By]
  - >> enter_isp

  lpcPHYStsPoll (Thumb, 148 bytes, Stack size 8 bytes, lpc_phy_smsc87x0.o(i.lpcPHYStsPoll))
  [Stack]

  - Max Depth = 8
  - Call Chain = lpcPHYStsPoll
  [Calls]
  - >> smsc_update_phy_sts
  - >> Chip_ENET_IsMIIBusy
  - >> Chip_ENET_StartMIIRead
  [Called By]
  - >> init_comms

  lpc_phy_init (Thumb, 172 bytes, Stack size 24 bytes, lpc_phy_smsc87x0.o(i.lpc_phy_init))
  [Stack]

  - Max Depth = 48
  - Call Chain = lpc_phy_init ⇒ lpc_mii_write
  [Calls]
  - >> lpc_mii_write
  - >> lpc_mii_read
  - >> Chip_GPIO_SetPinDIR
  [Called By]
  - >> init_comms

  main (Thumb, 26 bytes, Stack size 0 bytes, sbl_main.o(i.main))
  [Stack]

  - Max Depth = 192
  - Call Chain = main ⇒ enter_isp ⇒ isp_cmd_loop ⇒ exec_isp_cmd ⇒ write_to_ram ⇒ getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> user_code_present
  - >> execute_user_code
  - >> check_isp_entry_pin
  - >> enter_isp
  [Called By]
  - >> __rt_entry_main

  param_check (Thumb, 214 bytes, Stack size 36 bytes, isp_iap.o(i.param_check))
  [Stack]

  - Max Depth = 48
  - Call Chain = param_check ⇒ a_to_i
  [Calls]
  - >> is_div
  - >> a_to_i
  [Called By]
  - >> write_to_ram
  - >> unlock
  - >> read
  - >> prepare_sector
  - >> go_cmd
  - >> erase
  - >> copy
  - >> compare_mem
  - >> blank_check

  prepare_sector (Thumb, 118 bytes, Stack size 8 bytes, isp_iap.o(i.prepare_sector))
  [Stack]

  - Max Depth = 56
  - Call Chain = prepare_sector ⇒ param_check ⇒ a_to_i
  [Calls]
  - >> param_check
  - >> i_to_a
  - >> iap_entry
  - >> sendline_crlf
  [Called By]
  - >> exec_isp_cmd

  read (Thumb, 212 bytes, Stack size 48 bytes, isp_iap.o(i.read))
  [Stack]

  - Max Depth = 144
  - Call Chain = read ⇒ getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> uuencode
  - >> param_check
  - >> i_to_a
  - >> str_cmp
  - >> sendline_crlf
  - >> getline
  [Called By]
  - >> exec_isp_cmd

  sendline_crlf (Thumb, 332 bytes, Stack size 32 bytes, comms.o(i.sendline_crlf))
  [Stack]

  - Max Depth = 48
  - Call Chain = sendline_crlf ⇒ comms_process ⇒ ENET_TXBuffClaim
  [Calls]
  - >> comms_process
  - >> chksum16
  - >> incIndex
  - >> ENET_TXQueue
  [Called By]
  - >> write_to_ram
  - >> unlock
  - >> read
  - >> prepare_sector
  - >> go_cmd
  - >> exec_isp_cmd
  - >> erase
  - >> copy
  - >> compare_mem
  - >> blank_check
  - >> isp_cmd_loop
  - >> comm_handshake

  str_cmp (Thumb, 38 bytes, Stack size 8 bytes, isp_iap.o(i.str_cmp))
  [Stack]

  - Max Depth = 8
  - Call Chain = str_cmp
  [Called By]
  - >> read
  - >> comm_handshake

  tokenize (Thumb, 110 bytes, Stack size 28 bytes, isp_iap.o(i.tokenize))
  [Stack]

  - Max Depth = 28
  - Call Chain = tokenize
  [Called By]
  - >> isp_cmd_loop

  unlock (Thumb, 60 bytes, Stack size 16 bytes, isp_iap.o(i.unlock))
  [Stack]

  - Max Depth = 64
  - Call Chain = unlock ⇒ param_check ⇒ a_to_i
  [Calls]
  - >> param_check
  - >> i_to_a
  - >> sendline_crlf
  [Called By]
  - >> exec_isp_cmd

  user_code_present (Thumb, 40 bytes, Stack size 8 bytes, isp_iap.o(i.user_code_present))
  [Stack]

  - Max Depth = 24
  - Call Chain = user_code_present ⇒ iap_entry
  [Calls]
  - >> iap_entry
  [Called By]
  - >> main

  uudecode (Thumb, 202 bytes, Stack size 32 bytes, isp_iap.o(i.uudecode))
  [Stack]

  - Max Depth = 44
  - Call Chain = uudecode ⇒ decode_length
  [Calls]
  - >> decode_length
  - >> decode
  [Called By]
  - >> write_to_ram

  uuencode (Thumb, 136 bytes, Stack size 20 bytes, isp_iap.o(i.uuencode))
  [Stack]

  - Max Depth = 20
  - Call Chain = uuencode
  [Calls]
  - >> encode
  [Called By]
  - >> read

  write_to_ram (Thumb, 254 bytes, Stack size 48 bytes, isp_iap.o(i.write_to_ram))
  [Stack]

  - Max Depth = 144
  - Call Chain = write_to_ram ⇒ getline ⇒ getline_ex ⇒ Timer_HasTimestampExpired
  [Calls]
  - >> uudecode
  - >> param_check
  - >> i_to_a
  - >> a_to_i
  - >> sendline_crlf
  - >> getline
  [Called By]
  - >> exec_isp_cmd

  ### Local Symbols

  ENET_RXGet (Thumb, 102 bytes, Stack size 16 bytes, comms.o(i.ENET_RXGet))
  [Stack]

  - Max Depth = 16
  - Call Chain = ENET_RXGet
  [Calls]
  - >> incIndex
  [Called By]
  - >> getline_ex

  ENET_RXQueue (Thumb, 144 bytes, Stack size 16 bytes, comms.o(i.ENET_RXQueue))
  [Stack]

  - Max Depth = 16
  - Call Chain = ENET_RXQueue
  [Calls]
  - >> incIndex
  [Called By]
  - >> getline_ex
  - >> init_comms

  ENET_TXBuffClaim (Thumb, 74 bytes, Stack size 8 bytes, comms.o(i.ENET_TXBuffClaim))
  [Stack]

  - Max Depth = 8
  - Call Chain = ENET_TXBuffClaim
  [Calls]
  - >> incIndex
  [Called By]
  - >> comms_process

  ENET_TXQueue (Thumb, 170 bytes, Stack size 16 bytes, comms.o(i.ENET_TXQueue))
  [Stack]

  - Max Depth = 16
  - Call Chain = ENET_TXQueue
  [Calls]
  - >> incIndex
  [Called By]
  - >> sendline_crlf

  InitDescriptors (Thumb, 190 bytes, Stack size 24 bytes, comms.o(i.InitDescriptors))
  [Stack]

  - Max Depth = 28
  - Call Chain = InitDescriptors ⇒ __aeabi_memclr4
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> init_comms

  incIndex (Thumb, 10 bytes, Stack size 0 bytes, comms.o(i.incIndex))
  [Called By]

  - >> sendline_crlf
  - >> ENET_TXQueue
  - >> ENET_TXBuffClaim
  - >> ENET_RXQueue
  - >> ENET_RXGet

  localMsDelay (Thumb, 16 bytes, Stack size 0 bytes, comms.o(i.localMsDelay))
  [Address Reference Count : 1]

  - comms.o(i.init_comms)

  iap_entry (Thumb, 18 bytes, Stack size 16 bytes, isp_iap.o(i.iap_entry))
  [Stack]

  - Max Depth = 16
  - Call Chain = iap_entry
  [Called By]
  - >> prepare_sector
  - >> exec_isp_cmd
  - >> erase
  - >> copy
  - >> compare_mem
  - >> blank_check
  - >> user_code_present

  Chip_Clock_FindBaseClock (Thumb, 74 bytes, Stack size 8 bytes, clock_18xx_43xx.o(i.Chip_Clock_FindBaseClock))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_Clock_FindBaseClock
  [Called By]
  - >> Chip_Clock_GetRate

  Chip_Clock_GetDivRate (Thumb, 40 bytes, Stack size 24 bytes, clock_18xx_43xx.o(i.Chip_Clock_GetDivRate))
  [Stack]

  - Max Depth = 24 + In Cycle
  - Call Chain = Chip_Clock_GetDivRate ⇒ Chip_Clock_GetClockInputHz (Cycle)
  [Calls]
  - >> Chip_Clock_GetDividerSource
  - >> Chip_Clock_GetDividerDivisor
  - >> Chip_Clock_GetClockInputHz
  [Called By]
  - >> Chip_Clock_GetClockInputHz

  Chip_Clock_TestMainPLLMultiplier (Thumb, 26 bytes, Stack size 12 bytes, clock_18xx_43xx.o(i.Chip_Clock_TestMainPLLMultiplier))
  [Stack]

  - Max Depth = 12
  - Call Chain = Chip_Clock_TestMainPLLMultiplier
  [Called By]
  - >> Chip_Clock_SetupMainPLLHz

  convertTimmingParam (Thumb, 50 bytes, Stack size 12 bytes, emc_18xx_43xx.o(i.convertTimmingParam))
  [Stack]

  - Max Depth = 12
  - Call Chain = convertTimmingParam
  [Called By]
  - >> initStaticMem
  - >> initDynMem

  getColsLen (Thumb, 40 bytes, Stack size 0 bytes, emc_18xx_43xx.o(i.getColsLen))
  [Called By]

  - >> initDynMem

  Chip_TIMER_GetClockIndex (Thumb, 36 bytes, Stack size 0 bytes, timer_18xx_43xx.o(i.Chip_TIMER_GetClockIndex))
  [Called By]

  - >> Chip_TIMER_Init

  Board_LED_Init (Thumb, 48 bytes, Stack size 12 bytes, board.o(i.Board_LED_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = Board_LED_Init
  [Called By]
  - >> Board_Init

  Chip_SCU_PinMuxSet (Thumb, 12 bytes, Stack size 0 bytes, board.o(i.Chip_SCU_PinMuxSet))
  [Called By]

  - >> Board_Init

  Chip_SCU_SetPinMuxing (Thumb, 44 bytes, Stack size 16 bytes, board_sysinit.o(i.Chip_SCU_SetPinMuxing))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_SCU_SetPinMuxing
  [Called By]
  - >> Board_SetupMuxing

  Chip_ENET_IsMIIBusy (Thumb, 10 bytes, Stack size 0 bytes, lpc_phy_smsc87x0.o(i.Chip_ENET_IsMIIBusy))
  [Called By]

  - >> lpcPHYStsPoll
  - >> lpc_mii_write
  - >> lpc_mii_read

  lpc_mii_read (Thumb, 66 bytes, Stack size 24 bytes, lpc_phy_smsc87x0.o(i.lpc_mii_read))
  [Stack]

  - Max Depth = 24
  - Call Chain = lpc_mii_read
  [Calls]
  - >> Chip_ENET_IsMIIBusy
  - >> Chip_ENET_StartMIIRead
  [Called By]
  - >> lpc_phy_init

  lpc_mii_write (Thumb, 58 bytes, Stack size 24 bytes, lpc_phy_smsc87x0.o(i.lpc_mii_write))
  [Stack]

  - Max Depth = 24
  - Call Chain = lpc_mii_write
  [Calls]
  - >> Chip_ENET_IsMIIBusy
  - >> Chip_ENET_StartMIIWrite
  [Called By]
  - >> lpc_phy_init

  smsc_update_phy_sts (Thumb, 194 bytes, Stack size 0 bytes, lpc_phy_smsc87x0.o(i.smsc_update_phy_sts))
  [Called By]

  - >> lpcPHYStsPoll

  ### Undefined Global Symbols